IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2018-01-03T12:31:46"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140606_1530(x64) - Exporter 15.7.0.0 - Alternate UI 15.7.0.0"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "liam.needham" of Organization (no name given)
  Owner history of Person "liam.needham" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 1509111177 (2017-10-27T13:32:57Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCSLAB | object type "Floor:BSLTD_AProctorGroupLtd_FFT5ResilientOverlayShallowPlatformFloorSystem_ProfloorMicroDeck17" | FLOOR | names: "Floor:BSLTD_AProctorGroupLtd_FFT5ResilientOverlayShallowPlatformFloorSystem_ProfloorMicroDeck17:285987" | material: layers "Floor:BSLTD_AProctorGroupLtd_FFT5ResilientOverlayShallowPlatformFloorSystem_ProfloorMicroDeck17" ("BSLTD_AProctorGroupLtd_AcousticFlooring_ProfloorMicroDeck17" 17., "BSLTD_AProctorGroupLtd_GenericScreed" 65., "BSLTD_AProctorGroupLtd_GenericConcreteSlab" 200.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, NBS_General, COBie_Component, COBie_Warranty, COBie_Specification

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BSLTD_AProctorGroupLtd_FFT5ResilientOverlayShallowPlatformFloorSystem_ProfloorMicroDeck17" (IFCIDENTIFIER)
    ThermalTransmittance = 16.0923076923077 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "A Proctor Group" (IFCLABEL)
    ModelReference = "Profloor Micro Deck" (IFCLABEL)
  NBS_General | properties | on 1 object (1 IFCSLAB)
    Author = "BIM Strategy Ltd" (IFCTEXT)
    BIMObjectName = "BSLTD_AProctorGroupLtd_FFT5ResilientOverlayShallowPlatformFloorSystem_ProfloorMicroDeck17" (IFCTEXT)
    ManufacturerURL = "www.proctorgroup.com" (IFCTEXT)
    NBSDescription = "Wood floating floor system" (IFCTEXT)
    NBSReference = "20-55-95/195" (IFCTEXT)
    ProductInformation = "https://www.proctorgroup.com/products/profloor-micro-deck-17" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Ss_30_20_95_95" (IFCTEXT)
    Uniclass2015Title = "Wood floating floor systems" (IFCTEXT)
    Uniclass2015Version = "Systems v1.4" (IFCTEXT)
    Version = "1" (IFCTEXT)
  COBie_Component | properties | on 1 object (1 IFCSLAB)
    WarrantyStartDate = "31/12/1900/23:59:59" (IFCTEXT)
  COBie_Warranty | properties | on 1 object (1 IFCSLAB)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie_Specification | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "foam resilient layer, particleboard floor" (IFCTEXT)
    Features = "Ideal for situations where floor - to - ceiling height is critical (17mm total board depth), Deck is moisture resistant MDF, Panels have patented edge support strip which prevents fracture of the tongue and grooved joints" (IFCTEXT)
    Finish = "Moisture resistant Tongue and Groove MDF" (IFCTEXT)
    ModelReference = "Profloor Micro Deck" (IFCTEXT)
    Name = "BSLTD_AProctorGroupLtd_FFT5ResilientOverlayShallowPlatformFloorSystem_ProfloorMicroDeck17" (IFCTEXT)
    NominalHeight = 0. (IFCREAL)
    NominalLength = 0. (IFCREAL)
    NominalWidth = 0. (IFCREAL)
  COBie_ServiceLife | properties | on 1 object (1 IFCSLAB)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
  COBie_Asset | properties | on 1 object (1 IFCSLAB)
    AssetType = "fixed" (IFCTEXT)
  Pset_ManufacturerOccurance | properties | on 1 object (1 IFCSLAB)
    SerialNumber = "n/a" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)